MP4Box [option] input [option]
 -h general           general options help
 -h hint              hinting options help
 -h import            import options help
 -h encode            encode options help
 -h meta              meta handling options help
 -h extract           extraction options help
 -h dump              dump options help
 -h swf               Flash (SWF) options help
 -h crypt             ISMA E&A options help
 -h format            supported formats help
 -h rtp               streamer help

 -nodes               lists supported MPEG4 nodes
 -node NodeName       gets MPEG4 node syntax and QP info
 -xnodes              lists supported X3D nodes
 -xnode NodeName      gets X3D node syntax
 -snodes              lists supported SVG nodes
 -snode NodeName      gets SVG node syntax
 -languages           lists supported ISO 639 languages

-quiet                quiet mode
-noprog               disables progress
 -v                   verbose mode
 -version             gets build version
General Options:
 -inter time_in_ms    interleaves file data (track chunks of time_in_ms)
                       * Note 1: Interleaving is 0.5s by default
                       * Note 2: Performs drift checking accross tracks
                       * Note 3: a value of 0 disables interleaving
 -old-inter time      same as -inter but doesn't perform drift checking
 -tight               performs tight interleaving (sample based) of the file
                       * Note: reduces disk seek but increases file size
 -flat                stores file with all media data first, non-interleaved
 -frag time_in_ms     fragments file (track fragments of time_in_ms)
                       * Note: Always disables interleaving
 -ffspace size        inserts free space before moof in fragmented files
 -out filename        specifies output file name
                       * Note: By default input (MP4,3GP) file is overwritten
 -tmp dirname         specifies directory for temporary file creation
                       * Note: Default temp dir is OS-dependent
 -no-sys              removes all MPEG-4 Systems info except IOD (profiles)
                       * Note: Set by default whith '-add' and '-cat'
 -no-iod              removes InitialObjectDescriptor from file
 -isma                rewrites the file as an ISMA 1.0 AV file
 -ismax               same as '-isma' and removes all clock references
 -3gp                 rewrites as 3GPP(2) file (no more MPEG-4 Systems Info)
                       * Note 1: some tracks may be removed in the process
                       * Note 2: always on for *.3gp *.3g2 *.3gpp
 -ipod                rewrites the file for iPod
 -psp                 rewrites the file for PSP devices
 -brand ABCD[:v]      sets major brand of file, with optional version
 -ab ABCD             adds given brand to file's alternate brand list
 -rb ABCD             removes given brand from file's alternate brand list
 -cprt string         adds copyright string to movie
 -chap file           adds chapter information contained in file
 -rem trackID         removes track from file
 -enable trackID      enables track
 -disable trackID     disables track
 -new                 forces creation of a new destination file
 -rem trackID         removes track from file
 -lang [tkID=]LAN     sets track language. LAN is the ISO 639-2 code (eng, und)
 -delay tkID=TIME     sets track start delay in ms.
 -par tkID=PAR        sets visual track pixel aspect ratio (PAR=N:D or "none")
 -name tkID=NAME      sets track handler name
                       * NAME can indicate a UTF-8 file ("file://file name"
 -itags tag1[:tag2]   sets iTunes tags to file - more info: MP4Box -tag-list.
 -split time_sec      splits in files of time_sec max duration
                       * Note: this removes all MPEG-4 Systems media
 -split-size size     splits in files of max filesize kB.
                       * Note: this removes all MPEG-4 Systems media
 -split-chunk S:E     extracts a new file from Start to End (in seconds)
                       * Note: this removes all MPEG-4 Systems media
 -group-add fmt       creates a new grouping information in the file. Format is
                      a colon-separated list of following options:
                      refTrack=ID: ID of the track used as a group reference.
                       If not set, the track will belong to the same group as the previous trackID specified.
                       If 0 or no previous track specified, a new alternate group will be created
                      switchID=ID: ID of the switch group to create.
                       If 0, a new ID will be computed for you
                       If <0, disables SwitchGroup
                      criteria=string: list of space-separated 4CCs.
                      trackID=ID: ID of the track to add to this group.

                       *WARNING* Options modify state as they are parsed:
                        trackID=1:criteria=lang:trackID=2
                       is different from:
                        criteria=lang:trackID=1:trackID=2

 -group-rem-track ID  removes track from its group
 -group-rem ID        removes the track's group
 -group-clean         removes all group information from all tracks
 -ref id:XXXX:refID   adds a reference of type 4CC from track ID to track refID

 -dash dur            enables DASH-ing of the file with a segment duration of DUR
                       Note: the duration of a fragment (subsegment) is set
						using the interleaver (-inter) switch.
                       Note: You can specify -rap switch to split segments at RAP boundaries
 -frags-per-sidx N    sets the number of segments to be written in each SIDX box
                       If 0, SIDX box is not used
 -segment-name name   sets the segment name for generated segments
                       If not set (default), segments are concatenated in output file
 -segment-ext name    sets the segment extension. Default is m4s
 -url-template        uses UrlTemplate instead of explicit sources in segments.
                       Ignored if segments are stored in the output file.

Hinting Options
 -hint                hints the file for RTP/RTSP
 -mtu size            specifies RTP MTU (max size) in bytes. Default size is 1450
                       * Note: this includes the RTP header (12 bytes)
 -copy                copies media data to hint track rather than reference
                       * Note: speeds up server but takes much more space
 -multi [maxptime]    enables frame concatenation in RTP packets if possible
        maxptime       max packet duration in ms (optional, default 100ms)
 -rate ck_rate        specifies rtp rate in Hz when no default for payload
                       * Note: default value is 90000 (MPEG rtp rates)
 -mpeg4               forces MPEG-4 generic payload whenever possible
 -latm                forces MPG4-LATM transport for AAC streams
 -static              enables static RTP payload IDs whenever possible
                       * By default, dynamic payloads are always used

MPEG-4 Generic Payload Options
 -ocr                 forces all streams to be synchronized
                       * Most RTSP servers only support synchronized streams
 -rap                 signals random access points in RTP packets
 -ts                  signals AU Time Stamps in RTP packets
 -size                signals AU size in RTP packets
 -idx                 signals AU sequence numbers in RTP packets
 -iod                 prevents systems tracks embedding in IOD
                       * Note: shouldn't be used with -isma option

 -add-sdp string      adds sdp string to (hint) track ("-add-sdp tkID:string")
                       or movie. This will take care of SDP lines ordering
 -unhint              removes all hinting information.

Importing Options

File importing syntax:
 "#video" "#audio"  base import for most AV files
 "#trackID=ID"        track import for IsoMedia and other files
 "#pid=ID"            stream import from MPEG-2 TS
 ":dur=D"             imports only the first D seconds
 ":lang=LAN"          sets imported media language code
 ":delay=delay_ms"    sets imported media initial delay in ms
 ":par=PAR"           sets visual pixel aspect ratio (PAR=Num:Den)
 ":name=NAME"         sets track handler name
 ":ext=EXT"           overrides file extension when importing
 ":hdlr=code"         sets track handler type to the given code point (4CC)
 ":disable"           imported track(s) will be disabled
 ":group=G"           adds the track as part of the G alternate group.
                         If G is 0, the first available GroupID will be picked.
 ":fps=VAL"           same as -fps option
 ":agg=VAL"           same as -agg option
 ":par=VAL"           same as -par option
 ":dref"              same as -dref option
 ":nodrop"            same as -nodrop option
 ":packed"            same as -packed option
 ":sbr"               same as -sbr option
 ":sbrx"              same as -sbrx option
 ":ps":               same as -ps option
 ":psx":              same as -psx option
 ":ovsbr":            same as -ovsbr option
 ":mpeg4"             same as -mpeg4 option
 ":font=name"         specifies font name for text import (default "Serif")
 ":size=s"            specifies font size for text import (default 18)
 ":stype=4CC"         forces the sample description type to a different value
                         !! THIS MAY BREAK THE FILE WRITING !!
 ":chap"              specifies the track is a chapter track
 ":profile"           forces the profile for the H.264 content
                         - high444, high, extended, main, baseline
                         *WARNING* wrong value may cause playback issue
 ":compat"            forces the profile compatibity flags for the H.264 content
                         *WARNING* wrong value may cause playback issue
 ":level"             forces the level for the H.264 content
                         *Note: If value < 6, interpreted as decimal expression
 ":vidformat"         forces the video_format flag in VUI for the H.264 content
                         - component, pal, ntsc, secam, mac, undef
 ":fullrange"         forces the video_full_range_flag in VUI for the H.264 content
                         - on, off
 ":colorprim"         forces the colour_primaries flag in VUI for the H.264 content
                         - bt709, undef, bt470m, bt470bg, smpte170m, smpte240m, film
 ":transfer"          forces the transfer_characteristics flag in VUI for the H.264 content
                         - bt709, undef, bt470m, bt470bg, smpte170m, smpte240m, linear
                           log100, log316
 ":colmatrix"         forces the matrix_coefficients flag in VUI for the H.264 content
                         - GBR, bt709, undef, fcc, bt470bg, smpte170m, smpte240m, YCgCo
 ":layout=WxHxXxY"    specifies the track layout
                         - if W (resp H) = 0, the max width (resp height) of
                         the tracks in the file are used.
                         - if Y=-1, the layout is moved to the bottom of the
                         track area
                         - X and Y can be omitted (:layout=WxH)

 -add file              add file tracks to (new) output file
 -cat file              concatenates file samples to (new) output file
                         * Note: creates tracks if needed
 -force-cat             skips media configuration check when concatenating file
                         !!! THIS MAY BREAK THE CONCATENATED TRACK(S) !!!
 -keep-sys              keeps all MPEG-4 Systems info when using '-add' / 'cat'
 -keep-all              keeps all existing tracks when using '-add'
                         * Note: only used when adding IsoMedia files

All the following options can be specified as default or for each track.
When specified by track the syntax is ":opt" or ":opt=val".

 -dref                  keeps media data in original file
 -no-drop               forces constant FPS when importing AVI video
 -packed                forces packed bitstream when importing raw ASP
 -sbr                   backward compatible signaling of AAC-SBR
 -sbrx                  non-backward compatible signaling of AAC-SBR
 -ps:                   backward compatible signaling of AAC-PS
 -psx:                  non-backward compatible signaling of AAC-PS
 -ovsbr:                oversample SBR
                         * Note: SBR AAC, PS AAC and oversampled SBR cannot be detected at import time
 -fps FPS               forces frame rate for video and SUB subtitles import
                         FPS is either a number or expressed as timescale-increment
                         * For raw H263 import, default FPS is 15
                         * For all other imports, default FPS is 25
                         !! THIS IS IGNORED FOR IsoMedia IMPORT !!
 -mpeg4                 forces MPEG-4 sample descriptions when possible (3GPP2)
                         For AAC, forces MPEG-4 AAC signaling even if MPEG-2
 -agg N                 aggregates N audio frames in 1 sample (3GP media only)
                         * Note: Maximum value is 15 - Disabled by default

MPEG-4 Scene Encoding Options
 -mp4                 specify input file is for encoding.
 -def                 encode DEF names
 -sync time_in_ms     forces BIFS sync sample generation every time_in_ms
                       * Note: cannot be used with -shadow
 -shadow time_ms      forces BIFS sync shadow sample generation every time_ms.
                       * Note: cannot be used with -sync
 -log                 generates scene codec log file if available
 -ms file             specifies file for track importing

Chunk Processing
 -ctx-in file         specifies initial context (MP4/BT/XMT)
                       * Note: input file must be a commands-only file
 -ctx-out file        specifies storage of updated context (MP4/BT/XMT)

LASeR Encoding options
 -resolution res      resolution factor (-8 to 7, default 0)
                       all coords are multiplied by 2^res before truncation
 -coord-bits bits     bits used for encoding truncated coordinates
                       (0 to 31, default 12)
 -scale-bits bits     extra bits used for encoding truncated scales
                       (0 to 4, default 0)
 -auto-quant res      resolution is given as if using -resolution
                       but coord-bits and scale-bits are infered
Meta handling Options
 -set-meta args       sets given meta type - syntax: "ABCD[:tk=ID]"
                       * ABCD: four char meta type (NULL or 0 to remove meta)
                       * [:tk=ID]: if not set use root (file) meta
                                if ID is 0 use moov meta
                                if ID is not 0 use track meta
 -add-item args       adds resource to meta
                       * syntax: file_path + options (':' separated):
                        tk=ID: meta adressing (file, moov, track)
                        name=str: item name
                        mime=mtype: item mime type
                        encoding=enctype: item content-encoding type
                       * file_path "this" or "self": item is the file itself
 -rem-item args       removes resource from meta - syntax: item_ID[:tk=ID]
 -set-primary args    sets item as primary for meta - syntax: item_ID[:tk=ID]
 -set-xml args        sets meta XML data
                       * syntax: xml_file_path[:tk=ID][:binary]
 -rem-xml [tk=ID]     removes meta XML data
 -dump-xml args       dumps meta XML to file - syntax file_path[:tk=ID]
 -dump-item args      dumps item to file - syntax item_ID[:tk=ID][:path=fileName]
 -package             packages input XML file into an ISO container
                       * all media referenced except hyperlinks are added to file

Extracting Options
 -raw TrackID         extracts track in raw format when supported
 -raws TrackID        extract each track sample to a file
                       * Note: "TrackID:N" extracts Nth sample
 -nhnt TrackID        extracts track in nhnt format
 -nhml TrackID        extracts track in nhml format (XML nhnt).
                       * Note: "-nhml +TrackID" for full dump
 -single TrackID      extracts track to a new mp4 file
 -avi TrackID         extracts visual track to an avi file
 -qcp TrackID         same as '-raw' but defaults to QCP file for EVRC/SMV
 -aviraw TK           extracts AVI track in raw format
			            $TK can be one of "video" "audio" "audioN"
 -saf                 remux file to SAF multiplex
 -dvbhdemux           demux DVB-H file into IP Datagrams
                       * Note: can be used when encoding scene descriptions
 -diod                extracts file IOD in raw format when supported

Dumping Options
 -std                 dumps to stdout instead of file
 -info [trackID]      prints movie info / track info if trackID specified
                       * Note: for non IsoMedia files, gets import options
 -bt                  scene to bt format - removes unknown MPEG4 nodes
 -xmt                 scene to XMT-A format - removes unknown MPEG4 nodes
 -wrl                 scene VRML format - removes unknown VRML nodes
 -x3d                 scene to X3D/XML format - removes unknown X3D nodes
 -x3dv                scene to X3D/VRML format - removes unknown X3D nodes
 -lsr                 scene to LASeR format
 -diso                scene IsoMedia file boxes in XML output
 -drtp                rtp hint samples structure to XML output
 -dts                 prints sample timing to text output
 -sdp                 dumps SDP description of hinted file
 -dcr                 ISMACryp samples structure to XML output
 -dump-cover          Extracts cover art
 -dump-chap           Extracts chapter file

 -ttxt                Converts input subtitle to GPAC TTXT format
 -ttxt TrackID        Dumps Text track to GPAC TTXT format
 -srt                 Converts input subtitle to SRT format
 -srt TrackID         Dumps Text track to SRT format

 -stat                generates node/field statistics for scene
 -stats               generates node/field statistics per MPEG-4 Access Unit
 -statx               generates node/field statistics for scene after each AU

 -hash                generates SHA-1 Hash of the input file

SWF Importer Options

MP4Box can import simple Macromedia Flash files (".SWF")
You can specify a SWF input file with '-bt', 'xmt' and '-mp4' options

 -global              all SWF defines are placed in first scene replace
                       * Note: By default SWF defines are sent when needed
 -no-ctrl             uses a single stream for movie control and dictionary
                       * Note: this will disable ActionScript
 -no-text             removes all SWF text
 -no-font             removes all embedded SWF Fonts (terminal fonts used)
 -no-line             removes all lines from SWF shapes
 -no-grad             removes all gradients from swf shapes
 -quad                uses quadratic bezier curves instead of cubic ones
 -xlp                 support for lines transparency and scalability
 -flatten ang         complementary angle below which 2 lines are merged
                       * Note: angle '0' means no flattening

ISMA Encryption/Decryption Options
 -crypt drm_file      crypts a specific track using ISMA AES CTR 128
 -decrypt [drm_file]  decrypts a specific track using ISMA AES CTR 128
                       * Note: drm_file can be omitted if keys are in file
 -set-kms kms_uri     changes KMS location for all tracks or a given one.
                       * to adress a track, use 'tkID=kms_uri'

DRM file syntax for GPAC ISMACryp:
                      File is XML and shall start with xml header
                      File root is an "ISMACryp" element
                      File is a list of "ISMACrypTrack" elements

ISMACrypTrack attributes are
 TrackID              ID of track to en/decrypt
 key                  AES-128 key formatted (hex string '0x'+32 chars)
 salt                 CTR IV salt key (64 bits) (hex string '0x'+16 chars)

Encryption only attributes:
 Scheme_URI           URI of scheme used
 KMS_URI              URI of key management system
                       * Note: 'self' writes key and salt in the file
 selectiveType        selective encryption type - understood values are:
   "None"             all samples encrypted (default)
   "RAP"              only encrypts random access units
   "Non-RAP"          only encrypts non-random access units
   "Rand"             random selection is performed
   "X"                Encrypts every first sample out of X (uint)
   "RandX"            Encrypts one random sample out of X (uint)

 ipmpType             IPMP Signaling Type: None, IPMP, IPMPX
 ipmpDescriptorID     IPMP_Descriptor ID to use if IPMP(X) is used
                       * If not set MP4Box will generate one for you

Suppported raw formats and file extensions:
 NHNT                 .media .nhnt .info
 NHML                 .nhml (opt: .media .info)
 MPEG-1-2 Video       .m1v .m2v
 MPEG-4 Video         .cmp .m4v
 H263 Video           .263 .h263
 AVC/H264 Video       .h264 .h26L .264 .26L
 JPEG Images          .jpg .jpeg
 PNG Images           .png
 MPEG 1-2 Audio       .mp3, .m1a, .m2a
 ADTS-AAC Audio       .aac
 AMR(WB) Audio        .amr .awb
 EVRC Audio           .evc
 SMV Audio            .smv

Supported containers and file extensions:
 AVI                  .avi
 MPEG-2 PS            .mpg .mpeg .vob .vcd .svcd
 MPEG-2 TS            .ts .m2t
 QCP                  .qcp
 OGG                  .ogg
 ISO-Media files      no extension checking

Supported text formats:
 SRT Subtitles        .srt
 SUB Subtitles        .sub
 GPAC Timed Text      .ttxt
 QuickTime TeXML Text .xml  (cf QT documentation)

Supported Scene formats:
 MPEG-4 XMT-A         .xmt .xmta .xmt.gz .xmta.gz
 MPEG-4 BT            .bt .bt.gz
 VRML                 .wrl .wrl.gz
 X3D-XML              .x3d .x3d.gz
 X3D-VRML             .x3dv .x3dv.gz
 MacroMedia Flash     .swf (very limitted import support only)

File Streamer Options

MP4Box can stream ISO files to RTP. The streamer currently doesn't support
data carrouselling and will therefore not handle BIFS and OD streams properly.

-rtp         enables streamer
-noloop      disables looping when streaming
-mpeg4       forces MPEG-4 ES Generic for all RTP streams
-dst=IP      IP destination (uni/multi-cast). Default: 127.0.0.1
-port=PORT   output port of the first stream. Default: 7000
-mtu=MTU     path MTU for RTP packets. Default is 1450 bytes
-ifce=IFCE   IP address of the physical interface to use. Default: NULL (ANY)
-ttl=TTL     time to live for multicast packets. Default: 1
-sdp=Name    file name of the generated SDP. Default: "session.sdp"

Supported ISO 639 languages and codes:

Abkhazian (abk - ab)
Afar (aar - aa)
Afrikaans (afr - af)
Akan (aka - ak)
Albanian (sqi - sq)
Amharic (amh - am)
Arabic (ara - ar)
Aragonese (arg - an)
Armenian (hye - hy)
Assamese (asm - as)
Avaric (ava - av)
Avestan (ave - ae)
Aymara (aym - ay)
Azerbaijani (aze - az)
Bambara (bam - bm)
Bashkir (bak - ba)
Basque (eus - eu)
Belarusian (bel - be)
Bengali (ben - bn)
Bihari languages (bih - bh)
Bislama (bis - bi)
Bokmål, Norwegian; Norwegian Bokmål (nob - nb)
Bosnian (bos - bs)
Breton (bre - br)
Bulgarian (bul - bg)
Burmese (mya - my)
Catalan; Valencian (cat - ca)
Central Khmer (khm - km)
Chamorro (cha - ch)
Chechen (che - ce)
Chichewa; Chewa; Nyanja (nya - ny)
Chinese (zho - zh)
Church Slavic; Old Slavonic; Church Slavonic; Old Bulgarian; Old Church Slavonic (chu - cu)
Chuvash (chv - cv)
Cornish (cor - kw)
Corsican (cos - co)
Cree (cre - cr)
Croatian (hrv - hr)
Czech (ces - cs)
Danish (dan - da)
Divehi; Dhivehi; Maldivian (div - dv)
Dutch; Flemish (nld - nl)
Dzongkha (dzo - dz)
English (eng - en)
Esperanto (epo - eo)
Estonian (est - et)
Ewe (ewe - ee)
Faroese (fao - fo)
Fijian (fij - fj)
Finnish (fin - fi)
French (fra - fr)
Fulah (ful - ff)
Gaelic; Scottish Gaelic (gla - gd)
Galician (glg - gl)
Ganda (lug - lg)
Georgian (kat - ka)
German (deu - de)
Greek, Modern (1453-) (ell - el)
Guarani (grn - gn)
Gujarati (guj - gu)
Haitian; Haitian Creole (hat - ht)
Hausa (hau - ha)
Hebrew (heb - he)
Herero (her - hz)
Hindi (hin - hi)
Hiri Motu (hmo - ho)
Hungarian (hun - hu)
Icelandic (isl - is)
Ido (ido - io)
Igbo (ibo - ig)
Indonesian (ind - id)
Interlingua (International Auxiliary Language Association) (ina - ia)
Interlingue; Occidental (ile - ie)
Inuktitut (iku - iu)
Inupiaq (ipk - ik)
Irish (gle - ga)
Italian (ita - it)
Japanese (jpn - ja)
Javanese (jav - jv)
Kalaallisut; Greenlandic (kal - kl)
Kannada (kan - kn)
Kanuri (kau - kr)
Kashmiri (kas - ks)
Kazakh (kaz - kk)
Kikuyu; Gikuyu (kik - ki)
Kinyarwanda (kin - rw)
Kirghiz; Kyrgyz (kir - ky)
Komi (kom - kv)
Kongo (kon - kg)
Korean (kor - ko)
Kuanyama; Kwanyama (kua - kj)
Kurdish (kur - ku)
Lao (lao - lo)
Latin (lat - la)
Latvian (lav - lv)
Limburgan; Limburger; Limburgish (lim - li)
Lingala (lin - ln)
Lithuanian (lit - lt)
Luba-Katanga (lub - lu)
Luxembourgish; Letzeburgesch (ltz - lb)
Macedonian (mkd - mk)
Malagasy (mlg - mg)
Malay (msa - ms)
Malayalam (mal - ml)
Maltese (mlt - mt)
Manx (glv - gv)
Maori (mri - mi)
Marathi (mar - mr)
Marshallese (mah - mh)
Mongolian (mon - mn)
Nauru (nau - na)
Navajo; Navaho (nav - nv)
Ndebele, North; North Ndebele (nde - nd)
Ndebele, South; South Ndebele (nbl - nr)
Ndonga (ndo - ng)
Nepali (nep - ne)
Northern Sami (sme - se)
Norwegian (nor - no)
Norwegian Nynorsk; Nynorsk, Norwegian (nno - nn)
Occitan (post 1500) (oci - oc)
Ojibwa (oji - oj)
Oriya (ori - or)
Oromo (orm - om)
Ossetian; Ossetic (oss - os)
Pali (pli - pi)
Panjabi; Punjabi (pan - pa)
Persian (fas - fa)
Polish (pol - pl)
Portuguese (por - pt)
Pushto; Pashto (pus - ps)
Quechua (que - qu)
Romanian; Moldavian; Moldovan (ron - ro)
Romansh (roh - rm)
Rundi (run - rn)
Russian (rus - ru)
Samoan (smo - sm)
Sango (sag - sg)
Sanskrit (san - sa)
Sardinian (srd - sc)
Serbian (srp - sr)
Shona (sna - sn)
Sichuan Yi; Nuosu (iii - ii)
Sindhi (snd - sd)
Sinhala; Sinhalese (sin - si)
Slovak (slk - sk)
Slovenian (slv - sl)
Somali (som - so)
Sotho, Southern (sot - st)
Spanish; Castilian (spa - es)
Sundanese (sun - su)
Swahili (swa - sw)
Swati (ssw - ss)
Swedish (swe - sv)
Tagalog (tgl - tl)
Tahitian (tah - ty)
Tajik (tgk - tg)
Tamil (tam - ta)
Tatar (tat - tt)
Telugu (tel - te)
Thai (tha - th)
Tibetan (bod - bo)
Tigrinya (tir - ti)
Tonga (Tonga Islands) (ton - to)
Tsonga (tso - ts)
Tswana (tsn - tn)
Turkish (tur - tr)
Turkmen (tuk - tk)
Twi (twi - tw)
Uighur; Uyghur (uig - ug)
Ukrainian (ukr - uk)
Urdu (urd - ur)
Uzbek (uzb - uz)
Venda (ven - ve)
Vietnamese (vie - vi)
Volapük (vol - vo)
Walloon (wln - wa)
Welsh (cym - cy)
Western Frisian (fry - fy)
Wolof (wol - wo)
Xhosa (xho - xh)
Yiddish (yid - yi)
Yoruba (yor - yo)
Zhuang; Chuang (zha - za)
Zulu (zul - zu)
