Simple multimedia streams analyzer
usage: ffprobe [OPTIONS] [INPUT_FILE]

Main options:
-L                  show license
-h topic            show help
-? topic            show help
-help topic         show help
--help topic        show help
-version            show version
-buildconf          show build configuration
-formats            show available formats
-codecs             show available codecs
-decoders           show available decoders
-encoders           show available encoders
-bsfs               show available bit stream filters
-protocols          show available protocols
-filters            show available filters
-pix_fmts           show available pixel formats
-layouts            show standard channel layouts
-sample_fmts        show available audio sample formats
-colors             show available color names
-loglevel loglevel  set logging level
-v loglevel         set logging level
-report             generate a report
-max_alloc bytes    set maximum size of a single allocated block
-cpuflags flags     force specific cpu flags
-hide_banner hide_banner  do not show program banner
-f format           force format
-unit               show unit of the displayed values
-prefix             use SI prefixes for the displayed values
-byte_binary_prefix  use binary prefixes for byte units
-sexagesimal        use sexagesimal format HOURS:MM:SS.MICROSECONDS for time units
-pretty             prettify the format of displayed values, make it more human readable
-print_format format  set the output printing format (available formats are: default, compact, csv, flat, ini, json, xml)
-of format          alias for -print_format
-select_streams stream_specifier  select the specified streams
-sections           print sections structure and section information, and exit
-show_data          show packets data
-show_error         show probing error
-show_format        show format/container info
-show_frames        show frames info
-show_format_entry entry  show a particular entry from the format/container info
-show_entries entry_list  show a set of specified entries
-show_packets       show packets info
-show_programs      show programs info
-show_streams       show streams info
-show_chapters      show chapters info
-count_frames       count the number of frames per stream
-count_packets      count the number of packets per stream
-show_program_version  show ffprobe version
-show_library_versions  show library versions
-show_versions      show program and library versions
-show_private_data  show private data
-private            same as show_private_data
-bitexact           force bitexact output
-read_intervals read_intervals  set read intervals
-default            generic catch all option
-i input_file       read specified file


AVFormatContext AVOptions:
  -avioflags         <flags>      ED...... (default 0)
     direct                       ED...... reduce buffering
  -probesize         <int>        .D...... set probing size (from 32 to INT_MAX) (default 5e+006)
  -fflags            <flags>      ED...... (default 200)
     flush_packets                .D...... reduce the latency by flushing out packets immediately
     ignidx                       .D...... ignore index
     genpts                       .D...... generate pts
     nofillin                     .D...... do not fill in missing values that can be exactly calculated
     noparse                      .D...... disable AVParsers, this needs nofillin too
     igndts                       .D...... ignore dts
     discardcorrupt               .D...... discard corrupted frames
     sortdts                      .D...... try to interleave outputted packets by dts
     keepside                     .D...... don't merge side data
     nobuffer                     .D...... reduce the latency introduced by optional buffering
  -seek2any          <int>        .D...... allow seeking to non-keyframes on demuxer level when supported (from 0 to 1) (default 0)
  -analyzeduration   <int>        .D...... specify how many microseconds are analyzed to probe the input (from 0 to INT_MAX) (default 5e+006)
  -cryptokey         <binary>     .D...... decryption key
  -indexmem          <int>        .D...... max memory used for timestamp index (per stream) (from 0 to INT_MAX) (default 1.04858e+006)
  -rtbufsize         <int>        .D...... max memory used for buffering real-time frames (from 0 to INT_MAX) (default 3.04128e+006)
  -fdebug            <flags>      ED...... print specific debug info (default 0)
     ts                           ED......
  -max_delay         <int>        ED...... maximum muxing or demuxing delay in microseconds (from -1 to INT_MAX) (default -1)
  -fpsprobesize      <int>        .D...... number of frames used to probe fps (from -1 to 2.14748e+009) (default -1)
  -f_err_detect      <flags>      .D...... set error detection flags (deprecated; use err_detect, save via avconv) (default 1)
     crccheck                     .D...... verify embedded CRCs
     bitstream                    .D...... detect bitstream specification deviations
     buffer                       .D...... detect improper bitstream length
     explode                      .D...... abort decoding on minor error detection
     careful                      .D...... consider things that violate the spec, are fast to check and have not been seen in the wild as errors
     compliant                    .D...... consider all spec non compliancies as errors
     aggressive                   .D...... consider things that a sane encoder shouldn't do as an error
  -err_detect        <flags>      .D...... set error detection flags (default 1)
     crccheck                     .D...... verify embedded CRCs
     bitstream                    .D...... detect bitstream specification deviations
     buffer                       .D...... detect improper bitstream length
     explode                      .D...... abort decoding on minor error detection
     careful                      .D...... consider things that violate the spec, are fast to check and have not been seen in the wild as errors
     compliant                    .D...... consider all spec non compliancies as errors
     aggressive                   .D...... consider things that a sane encoder shouldn't do as an error
  -use_wallclock_as_timestamps <int>        .D...... use wallclock as timestamps (from 0 to 2.14748e+009) (default 0)
  -skip_initial_bytes <int>        .D...... set number of bytes to skip before reading header and frames (from 0 to 2.14748e+009) (default 0)
  -correct_ts_overflow <int>        .D...... correct single timestamp overflows (from 0 to 1) (default 1)

AVIOContext AVOptions:

URLContext AVOptions:

bluray AVOptions:
  -playlist          <int>        .D......  (from -1 to 99999) (default -1)
  -angle             <int>        .D......  (from 0 to 254) (default 0)
  -chapter           <int>        .D......  (from 1 to 65534) (default 1)

crypto AVOptions:
  -key               <binary>     .D...... AES decryption key
  -iv                <binary>     .D...... AES decryption initialization vector

file AVOptions:

ftp AVOptions:
  -timeout           <int>        ED...... set timeout of socket I/O operations (from -1 to INT_MAX) (default -1)
  -ftp-anonymous-password <string>     ED...... password for anonymous login. E-mail address should be used.

http AVOptions:
  -seekable          <int>        .D...... control seekability of connection (from -1 to 1) (default -1)
  -headers           <string>     ED...... set custom HTTP headers, can override built in default headers
  -content_type      <string>     ED...... set a specific content type for the POST messages
  -user_agent        <string>     .D...... override User-Agent header (default "Lavf/55.37.100")
  -user-agent        <string>     .D...... override User-Agent header (default "Lavf/55.37.100")
  -multiple_requests <int>        ED...... use persistent connections (from 0 to 1) (default 0)
  -post_data         <binary>     ED...... set custom HTTP post data
  -cookies           <string>     .D...... set cookies to be sent in applicable future requests, use newline delimited Set-Cookie HTTP field value syntax
  -icy               <int>        .D...... request ICY metadata (from 0 to 1) (default 0)
  -auth_type         <int>        ED...... HTTP authentication type (from 0 to 1) (default 0)
     none                         ED...... No auth method set, autodetect
     basic                        ED...... HTTP basic authentication
  -location          <string>     ED...... The actual location of the data received
  -offset            <int64>      .D...... initial byte offset (from 0 to I64_MAX) (default 0)
  -end_offset        <int64>      .D...... try to limit the request to bytes preceding this offset (from 0 to I64_MAX) (default 0)

https AVOptions:
  -seekable          <int>        .D...... control seekability of connection (from -1 to 1) (default -1)
  -headers           <string>     ED...... set custom HTTP headers, can override built in default headers
  -content_type      <string>     ED...... set a specific content type for the POST messages
  -user_agent        <string>     .D...... override User-Agent header (default "Lavf/55.37.100")
  -user-agent        <string>     .D...... override User-Agent header (default "Lavf/55.37.100")
  -multiple_requests <int>        ED...... use persistent connections (from 0 to 1) (default 0)
  -post_data         <binary>     ED...... set custom HTTP post data
  -cookies           <string>     .D...... set cookies to be sent in applicable future requests, use newline delimited Set-Cookie HTTP field value syntax
  -icy               <int>        .D...... request ICY metadata (from 0 to 1) (default 0)
  -auth_type         <int>        ED...... HTTP authentication type (from 0 to 1) (default 0)
     none                         ED...... No auth method set, autodetect
     basic                        ED...... HTTP basic authentication
  -location          <string>     ED...... The actual location of the data received
  -offset            <int64>      .D...... initial byte offset (from 0 to I64_MAX) (default 0)
  -end_offset        <int64>      .D...... try to limit the request to bytes preceding this offset (from 0 to I64_MAX) (default 0)

pipe AVOptions:

srtp AVOptions:

subfile AVOptions:
  -start             <int64>      .D...... start offset (from 0 to I64_MAX) (default 0)
  -end               <int64>      .D...... end offset (from 0 to I64_MAX) (default 0)

tcp AVOptions:
  -listen            <int>        ED...... listen on port instead of connecting (from 0 to 1) (default 0)
  -timeout           <int>        ED...... set timeout of socket I/O operations (from -1 to INT_MAX) (default -1)
  -listen_timeout    <int>        ED...... set connection awaiting timeout (from -1 to INT_MAX) (default -1)

tls AVOptions:
  -ca_file           <string>     ED...... Certificate Authority database file
  -cafile            <string>     ED...... Certificate Authority database file
  -tls_verify        <int>        ED...... Verify the peer certificate (from 0 to 1) (default 0)
  -cert_file         <string>     ED...... Certificate file
  -key_file          <string>     ED...... Private key file
  -listen            <int>        ED...... Listen for incoming connections (from 0 to 1) (default 0)

udp AVOptions:
  -buffer_size       <int>        ED...... set packet buffer size in bytes (from 0 to INT_MAX) (default 0)
  -localport         <int>        ED...... set local port to bind to (from 0 to INT_MAX) (default 0)
  -localaddr         <string>     ED...... choose local IP address (default "")
  -pkt_size          <int>        ED...... set size of UDP packets (from 0 to INT_MAX) (default 1472)
  -reuse             <int>        ED...... explicitly allow or disallow reusing UDP sockets (from 0 to 1) (default 0)
  -connect           <int>        ED...... set if connect() should be called on socket (from 0 to 1) (default 0)
  -fifo_size         <int>        .D...... set the UDP receiving circular buffer size, expressed as a number of packets with size of 188 bytes (from 0 to INT_MAX) (default 28672)
  -overrun_nonfatal  <int>        .D...... survive in case of UDP receiving circular buffer overrun (from 0 to 1) (default 0)
  -timeout           <int>        .D...... set raise error timeout (only in read mode) (from 0 to INT_MAX) (default 0)

librtmp protocol AVOptions:
  -rtmp_app          <string>     ED...... Name of application to connect to on the RTMP server
  -rtmp_playpath     <string>     ED...... Stream identifier to play or to publish

librtmpe protocol AVOptions:
  -rtmp_app          <string>     ED...... Name of application to connect to on the RTMP server
  -rtmp_playpath     <string>     ED...... Stream identifier to play or to publish

librtmps protocol AVOptions:
  -rtmp_app          <string>     ED...... Name of application to connect to on the RTMP server
  -rtmp_playpath     <string>     ED...... Stream identifier to play or to publish

librtmpt protocol AVOptions:
  -rtmp_app          <string>     ED...... Name of application to connect to on the RTMP server
  -rtmp_playpath     <string>     ED...... Stream identifier to play or to publish

librtmpte protocol AVOptions:
  -rtmp_app          <string>     ED...... Name of application to connect to on the RTMP server
  -rtmp_playpath     <string>     ED...... Stream identifier to play or to publish

Artworx Data Format demuxer AVOptions:
  -linespeed         <int>        .D...... set simulated line speed (bytes per second) (from 1 to INT_MAX) (default 6000)
  -video_size        <image_size> .D...... set video size, such as 640x480 or hd720.
  -framerate         <video_rate> .D...... set framerate (frames per second) (default "25")

aqtdec AVOptions:
  -subfps            <rational>   .D...S.. set the movie frame rate (from 0 to INT_MAX) (default 25/1)

asf demuxer AVOptions:
  -no_resync_search  <int>        .D...... Don't try to resynchronize by looking for a certain optional start code (from 0 to 1) (default 0)

avi AVOptions:
  -use_odml          <int>        .D...... use odml index (from -1 to 1) (default 1)

Binary text demuxer AVOptions:
  -linespeed         <int>        .D...... set simulated line speed (bytes per second) (from 1 to INT_MAX) (default 6000)
  -video_size        <image_size> .D...... set video size, such as 640x480 or hd720.
  -framerate         <video_rate> .D...... set framerate (frames per second) (default "25")

cavsvideo demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

CDXL demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 1 to INT_MAX) (default 11025)
  -framerate         <string>     .D...... 

concat demuxer AVOptions:
  -safe              <int>        .D...... enable safe mode (from -1 to 1) (default -1)

dirac demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

dnxhd demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

flvdec AVOptions:
  -flv_metadata      <int>        .D.V.... Allocate streams according to the onMetaData array (from 0 to 1) (default 0)

g729 demuxer AVOptions:
  -bit_rate          <int>        .D......  (from 0 to INT_MAX) (default 0)

GIF demuxer AVOptions:
  -min_delay         <int>        .D...... minimum valid delay between frames (in hundredths of second) (from 0 to 6000) (default 2)
  -default_delay     <int>        .D...... default delay between frames (in hundredths of second) (from 0 to 6000) (default 10)
  -ignore_loop       <int>        .D...... ignore loop setting (netscape extension) (from 0 to 1) (default 1)

gsm demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 1 to 6.50753e+007) (default 8000)

h261 demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

h263 demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

h264 demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

hevc demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

iCE Draw File demuxer AVOptions:
  -linespeed         <int>        .D...... set simulated line speed (bytes per second) (from 1 to INT_MAX) (default 6000)
  -video_size        <image_size> .D...... set video size, such as 640x480 or hd720.
  -framerate         <video_rate> .D...... set framerate (frames per second) (default "25")

image2 demuxer AVOptions:
  -framerate         <video_rate> .D...... set the video framerate (default "25")
  -loop              <int>        .D...... force loop over input file sequence (from 0 to 1) (default 0)
  -pattern_type      <int>        .D...... set pattern type (from 0 to INT_MAX) (default 0)
     glob_sequence                .D...... select glob/sequence pattern type
     glob                         .D...... select glob pattern type
     sequence                     .D...... select sequence pattern type
  -pixel_format      <string>     .D...... set video pixel format
  -start_number      <int>        .D...... set first number in the sequence (from 0 to INT_MAX) (default 0)
  -start_number_range <int>        .D...... set range for looking at the first sequence number (from 1 to INT_MAX) (default 5)
  -video_size        <image_size> .D...... set video size
  -frame_size        <int>        .D...... force frame size in bytes (from 0 to INT_MAX) (default 0)
  -ts_from_file      <int>        .D...... set frame timestamp from file's one (from 0 to 2) (default 0)
     none                         .D...... none
     sec                          .D...... second precision
     ns                           .D...... nano second precision

image2pipe demuxer AVOptions:
  -framerate         <video_rate> .D...... set the video framerate (default "25")
  -loop              <int>        .D...... force loop over input file sequence (from 0 to 1) (default 0)
  -pattern_type      <int>        .D...... set pattern type (from 0 to INT_MAX) (default 0)
     glob_sequence                .D...... select glob/sequence pattern type
     glob                         .D...... select glob pattern type
     sequence                     .D...... select sequence pattern type
  -pixel_format      <string>     .D...... set video pixel format
  -start_number      <int>        .D...... set first number in the sequence (from 0 to INT_MAX) (default 0)
  -start_number_range <int>        .D...... set range for looking at the first sequence number (from 1 to INT_MAX) (default 5)
  -video_size        <image_size> .D...... set video size
  -frame_size        <int>        .D...... force frame size in bytes (from 0 to INT_MAX) (default 0)
  -ts_from_file      <int>        .D...... set frame timestamp from file's one (from 0 to 2) (default 0)
     none                         .D...... none
     sec                          .D...... second precision
     ns                           .D...... nano second precision

ingenient demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

m4v demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

microdvddec AVOptions:
  -subfps            <rational>   .D...S.. set the movie frame rate fallback (from 0 to INT_MAX) (default 0/1)

mjpeg demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

mov,mp4,m4a,3gp,3g2,mj2 AVOptions:
  -use_absolute_path <int>        .D.V.... allow using absolute path when opening alias, this is a possible security issue (from 0 to 1) (default 0)
  -ignore_editlist   <int>        .D.V....  (from 0 to 1) (default 0)

mp3 AVOptions:
  -usetoc            <int>        .D...... use table of contents (from -1 to 1) (default -1)

mpegts demuxer AVOptions:
  -fix_teletext_pts  <int>        .D...... Try to fix pts values of dvb teletext streams. (from 0 to 1) (default 1)
  -ts_packetsize     <int>        .D....XR Output option carrying the raw packet size. (from 0 to 0) (default 0)

mpegtsraw demuxer AVOptions:
  -compute_pcr       <int>        .D...... Compute exact PCR for each transport stream packet. (from 0 to 1) (default 0)
  -ts_packetsize     <int>        .D....XR Output option carrying the raw packet size. (from 0 to 0) (default 0)

mpegvideo demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

alaw demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

mulaw demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

f64be demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

f64le demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

f32be demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

f32le demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

s32be demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

s32le demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

s24be demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

s24le demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

s16be demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

s16le demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

s8 demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

u32be demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

u32le demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

u24be demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

u24le demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

u16be demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

u16le demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

u8 demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D......  (from 0 to INT_MAX) (default 1)

rawvideo demuxer AVOptions:
  -video_size        <image_size> .D...... set frame size
  -pixel_format      <string>     .D...... set pixel format (default "yuv420p")
  -framerate         <video_rate> .D...... set frame rate (default "25")

RTP demuxer AVOptions:
  -rtp_flags         <flags>      .D...... set RTP flags (default 0)
     filter_src                   .D...... only receive packets from the negotiated peer IP
  -reorder_queue_size <int>        .D...... set number of packets to buffer for handling of reordered packets (from -1 to INT_MAX) (default -1)

RTSP demuxer AVOptions:
  -initial_pause     <int>        .D...... do not start playing the stream immediately (from 0 to 1) (default 0)
  -rtsp_transport    <flags>      ED...... set RTSP transport protocols (default 0)
     udp                          ED...... UDP
     tcp                          ED...... TCP
     udp_multicast                .D...... UDP multicast
     http                         .D...... HTTP tunneling
  -rtsp_flags        <flags>      .D...... set RTSP flags (default 0)
     filter_src                   .D...... only receive packets from the negotiated peer IP
     listen                       .D...... wait for incoming connections
     prefer_tcp                   ED...... try RTP via TCP first, if available
  -allowed_media_types <flags>      .D...... set media types to accept from the server (default 7)
     video                        .D...... Video
     audio                        .D...... Audio
     data                         .D...... Data
  -min_port          <int>        ED...... set minimum local UDP port (from 0 to 65535) (default 5000)
  -max_port          <int>        ED...... set maximum local UDP port (from 0 to 65535) (default 65000)
  -timeout           <int>        .D...... set maximum timeout (in seconds) to wait for incoming connections (-1 is infinite, imply flag listen) (from INT_MIN to INT_MAX) (default -1)
  -stimeout          <int>        .D...... set timeout (in micro seconds) of socket TCP I/O operations (from INT_MIN to INT_MAX) (default 0)
  -reorder_queue_size <int>        .D...... set number of packets to buffer for handling of reordered packets (from -1 to INT_MAX) (default -1)
  -user-agent        <string>     .D...... override User-Agent header (default "Lavf55.37.100")

sbg_demuxer AVOptions:
  -sample_rate       <int>        .D......  (from 0 to INT_MAX) (default 0)
  -frame_size        <int>        .D......  (from 0 to INT_MAX) (default 0)
  -max_file_size     <int>        .D......  (from 0 to INT_MAX) (default 5e+006)

SDP demuxer AVOptions:
  -sdp_flags         <flags>      .D...... SDP flags (default 0)
     filter_src                   .D...... only receive packets from the negotiated peer IP
     custom_io                    .D...... use custom I/O
     rtcp_to_source               .D...... send RTCP packets to the source address of received packets
  -allowed_media_types <flags>      .D...... set media types to accept from the server (default 7)
     video                        .D...... Video
     audio                        .D...... Audio
     data                         .D...... Data
  -reorder_queue_size <int>        .D...... set number of packets to buffer for handling of reordered packets (from -1 to INT_MAX) (default -1)

tedcaptions_demuxer AVOptions:
  -start_time        <int64>      .D...S.. set the start time (offset) of the subtitles, in ms (from I64_MIN to I64_MAX) (default 15000)

TTY demuxer AVOptions:
  -chars_per_frame   <int>        .D......  (from 1 to INT_MAX) (default 6000)
  -video_size        <image_size> .D...... A string describing frame size, such as 640x480 or hd720.
  -framerate         <video_rate> .D......  (default "25")

vc1 demuxer AVOptions:
  -framerate         <video_rate> .D......  (default "25")

WAV demuxer AVOptions:
  -ignore_length     <int>        .D...... Ignore length (from 0 to 1) (default 0)

WebVTT demuxer AVOptions:

eXtended BINary text (XBIN) demuxer AVOptions:
  -linespeed         <int>        .D...... set simulated line speed (bytes per second) (from 1 to INT_MAX) (default 6000)
  -video_size        <image_size> .D...... set video size, such as 640x480 or hd720.
  -framerate         <video_rate> .D...... set framerate (frames per second) (default "25")

ModPlug demuxer AVOptions:
  -noise_reduction   <int>        .D...... Enable noise reduction 0(off)-1(on) (from 0 to 1) (default 0)
  -reverb_depth      <int>        .D...... Reverb level 0(quiet)-100(loud) (from 0 to 100) (default 0)
  -reverb_delay      <int>        .D...... Reverb delay in ms, usually 40-200ms (from 0 to INT_MAX) (default 0)
  -bass_amount       <int>        .D...... XBass level 0(quiet)-100(loud) (from 0 to 100) (default 0)
  -bass_range        <int>        .D...... XBass cutoff in Hz 10-100 (from 0 to 100) (default 0)
  -surround_depth    <int>        .D...... Surround level 0(quiet)-100(heavy) (from 0 to 100) (default 0)
  -surround_delay    <int>        .D...... Surround delay in ms, usually 5-40ms (from 0 to INT_MAX) (default 0)
  -max_size          <int>        .D...... Max file size supported (in bytes). Default is 5MB. Set to 0 for no limit (not recommended) (from 0 to 1.04858e+008) (default 5.24288e+006)
  -video_stream_expr <string>     .D...... Color formula
  -video_stream      <int>        .D...... Make demuxer output a video stream (from 0 to 1) (default 0)
  -video_stream_w    <int>        .D...... Video stream width in char (one char = 8x8px) (from 20 to 512) (default 30)
  -video_stream_h    <int>        .D...... Video stream height in char (one char = 8x8px) (from 20 to 512) (default 30)
  -video_stream_ptxt <int>        .D...... Print speed, tempo, order, ... in video stream (from 0 to 1) (default 1)

dshow indev AVOptions:
  -video_size        <image_size> .D...... set video size given a string such as 640x480 or hd720.
  -pixel_format      <pix_fmt>    .D...... set video pixel format (default none)
  -framerate         <string>     .D...... set video frame rate
  -sample_rate       <int>        .D...... set audio sample rate (from 0 to INT_MAX) (default 0)
  -sample_size       <int>        .D...... set audio sample size (from 0 to 16) (default 0)
  -channels          <int>        .D...... set number of audio channels, such as 1 or 2 (from 0 to INT_MAX) (default 0)
  -list_devices      <int>        .D...... list available devices (from 0 to 1) (default 0)
     true                         .D...... 
     false                        .D...... 
  -list_options      <int>        .D...... list available options for specified device (from 0 to 1) (default 0)
     true                         .D...... 
     false                        .D...... 
  -video_device_number <int>        .D...... set video device number for devices with same name (starts at 0) (from 0 to INT_MAX) (default 0)
  -audio_device_number <int>        .D...... set audio device number for devices with same name (starts at 0) (from 0 to INT_MAX) (default 0)
  -audio_buffer_size <int>        .D...... set audio device buffer latency size in milliseconds (default is the device's default) (from 0 to INT_MAX) (default 0)

GDIgrab indev AVOptions:
  -draw_mouse        <int>        .D...... draw the mouse pointer (from 0 to 1) (default 1)
  -show_region       <int>        .D...... draw border around capture area (from 0 to 1) (default 0)
  -framerate         <video_rate> .D...... set video frame rate (default "ntsc")
  -video_size        <image_size> .D...... set video frame size
  -offset_x          <int>        .D...... capture area x offset (from INT_MIN to INT_MAX) (default 0)
  -offset_y          <int>        .D...... capture area y offset (from INT_MIN to INT_MAX) (default 0)

lavfi indev AVOptions:
  -graph             <string>     .D...... set libavfilter graph
  -graph_file        <string>     .D...... set libavfilter graph filename
  -dumpgraph         <string>     .D...... dump graph to stderr

VFW indev AVOptions:
  -video_size        <string>     .D...... A string describing frame size, such as 640x480 or hd720.
  -framerate         <string>     .D......  (default "ntsc")

ADTS muxer AVOptions:

AIFF muxer AVOptions:

AST muxer AVOptions:

f4v muxer AVOptions:

flac muxer AVOptions:

frame hash encoder class AVOptions:

GIF muxer AVOptions:

HDS muxer AVOptions:

hls muxer AVOptions:

image2 muxer AVOptions:

ipod muxer AVOptions:

ismv muxer AVOptions:

LATM/LOAS muxer AVOptions:

hash encoder class AVOptions:

matroska muxer AVOptions:

matroska audio muxer AVOptions:

mov muxer AVOptions:

MP3 muxer AVOptions:

mp4 muxer AVOptions:

mpeg muxer AVOptions:

vcd muxer AVOptions:

dvd muxer AVOptions:

svcd muxer AVOptions:

vob muxer AVOptions:

MPEGTS muxer AVOptions:

Ogg audio muxer AVOptions:

Ogg muxer AVOptions:

Opus muxer AVOptions:

psp muxer AVOptions:

RTP muxer AVOptions:

RTSP muxer AVOptions:
  -initial_pause     <int>        .D...... do not start playing the stream immediately (from 0 to 1) (default 0)
  -rtsp_transport    <flags>      ED...... set RTSP transport protocols (default 0)
     udp                          ED...... UDP
     tcp                          ED...... TCP
     udp_multicast                .D...... UDP multicast
     http                         .D...... HTTP tunneling
  -rtsp_flags        <flags>      .D...... set RTSP flags (default 0)
     filter_src                   .D...... only receive packets from the negotiated peer IP
     listen                       .D...... wait for incoming connections
     prefer_tcp                   ED...... try RTP via TCP first, if available
  -allowed_media_types <flags>      .D...... set media types to accept from the server (default 7)
     video                        .D...... Video
     audio                        .D...... Audio
     data                         .D...... Data
  -min_port          <int>        ED...... set minimum local UDP port (from 0 to 65535) (default 5000)
  -max_port          <int>        ED...... set maximum local UDP port (from 0 to 65535) (default 65000)
  -timeout           <int>        .D...... set maximum timeout (in seconds) to wait for incoming connections (-1 is infinite, imply flag listen) (from INT_MIN to INT_MAX) (default -1)
  -stimeout          <int>        .D...... set timeout (in micro seconds) of socket TCP I/O operations (from INT_MIN to INT_MAX) (default 0)
  -reorder_queue_size <int>        .D...... set number of packets to buffer for handling of reordered packets (from -1 to INT_MAX) (default -1)
  -user-agent        <string>     .D...... override User-Agent header (default "Lavf55.37.100")

segment muxer AVOptions:

stream_segment muxer AVOptions:

smooth streaming muxer AVOptions:

spdif AVOptions:

Speex muxer AVOptions:

tg2 muxer AVOptions:

tgp muxer AVOptions:

WAV muxer AVOptions:

webm muxer AVOptions:

caca_outdev AVOptions:

sdl outdev AVOptions:

