
2011. svibanj 15  11:17:52 CEST
ProjectX 0.90.4.00.b25 (07.09.2008)

-> working with collection 0
 
-> save normal log file
-> log 'packets out of sequence' / bit errors
-> log 'missing startcodes'
-> log 'PES header found in ES'
-> log WSS
-> log VPS
-> log RDS
-> log max. 500 warnings/errors
-> write all video data
-> write all other data
-> patch c.d.flagged infos of pictures
-> add sequence end code
-> set resolution in SDE 
-> PVA: strictly specs. for audio streams
-> VOB: determine diff. Cell timelines
-> TS: ignore scrambled packets
-> TS: enhanced search for open packets
-> TS: join file segments (of Dreambox®)
-> TS: generate PMT stream dependent
-> get only enclosed PES/TS packets
-> concatenate different recordings
-> ensure 1st PES-packet start with video
-> generate PCR/SCR from PTS
 
-> write output files to: 'D:\DVB-T'

-> main I/O-Buffersize in bytes 4096000 bytes

FileSegments:
* (0) D:\DVB-T\000.0000.ts
* (1) D:\DVB-T\001.0000.ts
second. Files:
* ---

+> Input File 0:  'D:\DVB-T\000.0000.ts' (97.930.140 bytes)
-> Filetype is TS (generic PES Container)
-> demux
-> Service ID 0x1
-> PMT 0x10 refers to these usable streams:
Video:
PID: 0x11
Audio:
PID: 0x14(hrv)
Teletext:
n/a
Subpict.:
n/a

!> PID 0x0 (PAT) (0 #1) -> ignored
!> PID 0x10 (PMT) (564 #4) -> ignored
ok> PID 0x11 has PES-ID 0xE0 (MPEG Video) (940 #6) 
ok> PID 0x14 has PES-ID 0xC0 (MPEG Audio) (79524 #424) 
-> video basics: 720*576 @ 25fps @ 0.6735 (4:3) @ 4600000bps, vbvBuffer 112
-> starting export of video data @ GOP# 0
!> dropping useless B-Frames @ GOP# 0 / new Timecode 00:00:00.000
-> actual written vframes: 3901
switch to file: D:\DVB-T\001.0000.ts (44.867.704 bytes) @ 97930140
!> PID 0x11 -> packet 520911 @ pos. 97931080 out of sequence (0/5) (shifting counter..) (~00:02:36.040)
!> PID 0x14 -> packet 520924 @ pos. 97933524 out of sequence (0/8) (shifting counter..) (~00:02:36.040)
!> dropping GOP# 326 @ orig.PTS 00:36:16.788 (195911005), errorcode: 24
!> Pics exp/cnt 3/1, inGOP PTS diff. 0ms, new Timecode 00:02:36.520
packs: 758565 100% 142797844

++> Mpg Video: PID 0x0011 / PesID 0xE0 / SubID 0x00 :
-> Video: fr-ct-1p-cg-og-dg -> 5701-1-1-475-0-1
-> Video length: 5701 frames @ 00:03:48.040
-> GOP summary: min. 12, max. 36 fields; contains interlaced frames
-> avg. nom. bitrate 4616516bps (min/max: 2750000/6919200)
-> set first sequenceheader bitrate to 6919200bps
---> new File: D:\DVB-T\000.0000.m2v

++> Mpg Audio: PID 0x0014 / PesID 0xC0 / SubID 0x00 :
-> Audio: limit points of PTS for sync
-> check CRC of AC-3 / MPEG-Audio L1,2
-> remove CRC in MPEG-Audio L1,2
-> fill gaps with prev. frame
-> add frames
-> Audio PTS: first packet 00:33:40.091, last packet 00:37:28.187
-> Video PTS: start 1.GOP 00:33:40.268, end last GOP 00:37:28.308
-> adjusting audio at video-timeline
-> src_audio: MPEG-1, Layer2, 48000Hz, stereo, 256kbps, CRC @ 00:00:00.000
!> missing syncword @  5010433, @ 00:02:36.408
!> found syncword @ 5011288
!> missing syncword @  5012825, @ 00:02:36.456
!> found syncword @ 5013504
!> 3 frame(s) (72ms) inserted @ 00:02:36.624
audio frames: wri-pre-skip-ins-add 9502-0-0-3-0 @ 00:03:48.048 done...
---> new File: 'D:\DVB-T\000.0000.mp2'

summary of created media files:
.Video (m2v):	5701 Frames	00:03:48.040		'D:\DVB-T\000.0000.m2v'
Audio 00 (mp2):	9502 Frames	00:03:48.048	0-0-3-0	'D:\DVB-T\000.0000.mp2'
=> 138.891.332 bytes written...
-> we have 12 warnings/errors.