FFmpeg version CVS, Copyright (c) 2000-2004 Fabrice Bellard
Mac OSX universal build for ffmpegX
  configuration:  --enable-memalign-hack --enable-mp3lame --enable-gpl --disable-vhook --disable-ffplay --disable-ffserver --enable-a52 --enable-xvid --enable-faac --enable-faad --enable-amr_nb --enable-amr_wb --enable-pthreads --enable-x264 
  libavutil version: 49.0.0
  libavcodec version: 51.9.0
  libavformat version: 50.4.0
  built on Apr 15 2006 04:58:19, gcc: 4.0.1 (Apple Computer, Inc. build 5250)
Input #0, mp3, from '/Users/tory/Desktop/AZatCal/C.mpg-0.mp2':
  Duration: 00:05:36.3, start: 0.000000, bitrate: 112 kb/s
  Stream #0.0: Audio: mp2, 48000 Hz, mono, 112 kb/s
Output #0, mp2, to '/Users/tory/Desktop/AZatCal/C.mpg-0.s.mp2':
  Stream #0.0: Audio: mp2, 48000 Hz, stereo, 224 kb/s
Stream mapping:
  Stream #0.0 -> #0.0
video:0kB audio:9191kB global headers:0kB muxing overhead 0.000000%
   INFO: [mplex] mplex version 1.9.0 (2.2.7 $Date: 2006/02/01 22:23:01 $)
   INFO: [mplex] File /Users/tory/Desktop/AZatCal/C.mpg-0.m2v looks like an MPEG Video stream.
   INFO: [mplex] File /Users/tory/Desktop/AZatCal/C.mpg-0.s.mp2 looks like an MPEG Audio stream.
   INFO: [mplex] Video stream 0: profile 8 selected - ignoring non-standard options!
   INFO: [mplex] Found 1 audio streams and 1 video streams
   INFO: [mplex] Selecting dvdauthor DVD output profile
   INFO: [mplex] Multiplexing video program stream!
   INFO: [mplex] Scanning for header info: Video stream e0 (/Users/tory/Desktop/AZatCal/C.mpg-0.m2v) 
   INFO: [mplex] VIDEO STREAM: e0
   INFO: [mplex] Frame width     : 720
   INFO: [mplex] Frame height    : 480
   INFO: [mplex] Aspect ratio    : 4:3 display
   INFO: [mplex] Picture rate    : 29.970 frames/sec
   INFO: [mplex] Bit rate        : 8000000 bits/sec
   INFO: [mplex] Vbv buffer size : 229376 bytes
   INFO: [mplex] CSPF            : 0
   INFO: [mplex] Scanning for header info: Audio stream c0 (/Users/tory/Desktop/AZatCal/C.mpg-0.s.mp2)
   INFO: [mplex] MPEG AUDIO STREAM: c0
   INFO: [mplex] Audio version  : 1.0
   INFO: [mplex] Layer          :        2
   INFO: [mplex] CRC checksums  :       no
   INFO: [mplex] Bit rate       :    28672 bytes/sec (224 kbit/sec)
   INFO: [mplex] Frequency      :     48000 Hz
   INFO: [mplex] Mode           :        0 stereo
   INFO: [mplex] Mode extension :        0
   INFO: [mplex] Copyright bit  :        0 no copyright
   INFO: [mplex] Original/Copy  :        1 original
   INFO: [mplex] Emphasis       :        0 none
   INFO: [mplex] SYSTEMS/PROGRAM stream:
   INFO: [mplex] rough-guess multiplexed stream data rate    : 8399296
   INFO: [mplex] target data-rate specified               : 10080000
   INFO: [mplex] Setting specified specified data rate: 10080000
   INFO: [mplex] Run-in delay = 9009 Video delay = 9009 Audio delay = 12012
   INFO: [mplex] New sequence commences...
++ WARN: [mplex] Stream e0: data will arrive too late sent(SCR)=27955492 required(DTS)=9009
   INFO: [mplex] STREAM c0 completed @ frame 14004.
   INFO: [mplex] STREAM e0 completed @ frame 10431.
   INFO: [mplex] Multiplex completion at SCR=31317284.
   INFO: [mplex] VIDEO_STATISTICS: e0
   INFO: [mplex] Video Stream length:   136291220 bytes
   INFO: [mplex] Sequence headers:      352
   INFO: [mplex] Sequence ends   :        0
   INFO: [mplex] No. Pictures    :    10432
   INFO: [mplex] No. Groups      :      351
   INFO: [mplex] No. I Frames    :      351 avg. size 33757 bytes
   INFO: [mplex] No. P Frames    :     3867 avg. size 18624 bytes
   INFO: [mplex] No. B Frames    :     6150 avg. size  8372 bytes
   INFO: [mplex] Average bit-rate :  3127600 bits/sec
   INFO: [mplex] Peak bit-rate    :  7043200  bits/sec
   INFO: [mplex] BUFFERING min 15 Buf max 216789
   INFO: [mplex] AUDIO_STATISTICS: c0
   INFO: [mplex] Audio stream length 9411360 bytes.
   INFO: [mplex] Syncwords      :    14005
   INFO: [mplex] Frames         :    14005 padded
   INFO: [mplex] Frames         :        0 unpadded
   INFO: [mplex] BUFFERING min 15 Buf max 683
**ERROR: [mplex] MUX STATUS: Frame data under-runs detected!